1. Finished the sensitivity analysis in Kriging-PMO
2. Create a new way in updating the cut center
   1. When f\_0\_new is bigger than f\_0\_old, remain x\_0\_old, i.e. x\_0\_new won’t be updated.